<!DOCTYPE PATCH  SYSTEM "http://vvvv.org/versions/vvvv33beta13.1.dtd" >
   <PATCH nodename="C:\Dokumente und Einstellungen\MESO\Desktop\vvvv_33beta13.1\vvvv_33beta13.1\help\IO (Devices Wiesemann+Theis Digital-EA) help.v4p">
   <BOUNDS height="7530" left="285" top="540" type="Window" width="12315">
   </BOUNDS>
   <NODE componentmode="InABox" id="10" nodename="IOBox (String)">
   <BOUNDS height="270" left="45" top="60" type="Node" width="2535">
   </BOUNDS>
   <BOUNDS height="435" left="45" top="60" type="Box" width="5475">
   </BOUNDS>
   <BOUNDS height="160" left="300" top="300" type="Window" width="215">
   </BOUNDS>
   <PIN pinname="Input String" slicecount="1" visible="0" values="|IO (Devices Wiesemann+Theis Digital-EA)|">
   </PIN>
   <PIN pinname="Output String" visible="0">
   </PIN>
   <PIN pinname="Show Grid" slicecount="1" values="0">
   </PIN>
   <PIN pinname="Size" slicecount="1" values="12">
   </PIN>
   </NODE>
   <NODE componentmode="InABox" id="9" nodename="IOBox (String)">
   <BOUNDS height="270" left="45" top="495" type="Node" width="1665">
   </BOUNDS>
   <BOUNDS height="360" left="45" top="495" type="Box" width="4395">
   </BOUNDS>
   <BOUNDS height="160" left="300" top="300" type="Window" width="215">
   </BOUNDS>
   <PIN pinname="Input String" slicecount="1" visible="0" values="|Connect Wiesemann+Theis Digital-EA or Web-IO to VVVV|">
   </PIN>
   <PIN pinname="Output String" visible="0">
   </PIN>
   <PIN pinname="Show Grid" slicecount="1" values="0">
   </PIN>
   </NODE>
   <NODE componentmode="InABox" id="8" nodename="IOBox (String)">
   <BOUNDS height="270" left="885" top="5280" type="Node" width="3960">
   </BOUNDS>
   <BOUNDS height="1590" left="885" top="5280" type="Box" width="4920">
   </BOUNDS>
   <BOUNDS height="160" left="0" top="0" type="Window" width="215">
   </BOUNDS>
   <PIN pinname="Input String" slicecount="1" visible="0" values="|set the IP Address pin to match the IP Address of the target device. &cr;&lf;&cr;&lf;the default TCP Port 49153 is the default used by W&amp;T devices, so only change this pin if a different port number has been configured on the W&amp;T box. &cr;&lf;&cr;&lf;you can only have one node for each device connected in vvvv. |">
   </PIN>
   <PIN pinname="Output String" visible="0">
   </PIN>
   <PIN pinname="Show Grid" slicecount="1" values="0">
   </PIN>
   </NODE>
   <NODE id="7" nodename="IO (Devices Wiesemann+Theis Digital-EA)">
   <BOUNDS height="270" left="3540" top="3570" type="Node" width="1935">
   </BOUNDS>
   <PIN pinname="Connected" visible="1">
   </PIN>
   <PIN pinname="Output" visible="1">
   </PIN>
   <PIN pinname="Input" visible="1">
   </PIN>
   <PIN pinname="IP Address" visible="1">
   </PIN>
   <PIN pinname="Enabled" slicecount="1" values="1">
   </PIN>
   </NODE>
   <NODE componentmode="InABox" id="6" nodename="IOBox (Value Advanced)">
   <BOUNDS height="0" left="450" top="4080" type="Node" width="0">
   </BOUNDS>
   <BOUNDS height="160" left="7320" top="16245" type="Window" width="215">
   </BOUNDS>
   <BOUNDS height="300" left="450" top="4080" type="Box" width="3150">
   </BOUNDS>
   <PIN pinname="Show Value" slicecount="1" values="0">
   </PIN>
   <PIN pinname="Show Slider" slicecount="1" values="1">
   </PIN>
   <PIN pinname="Minimum" slicecount="1" values="0">
   </PIN>
   <PIN pinname="Maximum" slicecount="1" values="1">
   </PIN>
   <PIN pinname="Slider Behavior" slicecount="1" values="Toggle">
   </PIN>
   <PIN pinname="Y Input Value" visible="1">
   </PIN>
   <PIN pinname="Columns" slicecount="1" values="12">
   </PIN>
   <PIN pinname="SliceCount Mode" slicecount="1" values="ColsRowsPages">
   </PIN>
   <PIN pinname="Y Output Value" visible="1">
   </PIN>
   </NODE>
   <NODE componentmode="InABox" id="5" nodename="IOBox (Value Advanced)">
   <BOUNDS height="0" left="5040" top="4035" type="Node" width="0">
   </BOUNDS>
   <BOUNDS height="160" left="11175" top="8430" type="Window" width="215">
   </BOUNDS>
   <BOUNDS height="390" left="5040" top="4035" type="Box" width="450">
   </BOUNDS>
   <PIN pinname="Y Output Value" visible="1">
   </PIN>
   <PIN pinname="Y Input Value" visible="1">
   </PIN>
   <PIN pinname="Show Slider" slicecount="1" values="1">
   </PIN>
   <PIN pinname="Show Value" slicecount="1" values="0">
   </PIN>
   <PIN pinname="Slider Behavior" slicecount="1" values="Toggle">
   </PIN>
   <PIN pinname="Minimum" slicecount="1" values="0">
   </PIN>
   <PIN pinname="Maximum" slicecount="1" values="1">
   </PIN>
   </NODE>
   <NODE componentmode="InABox" id="4" nodename="IOBox (String)">
   <BOUNDS height="270" left="4845" top="4440" type="Node" width="930">
   </BOUNDS>
   <BOUNDS height="240" left="4845" top="4440" type="Box" width="825">
   </BOUNDS>
   <BOUNDS height="160" left="300" top="300" type="Window" width="215">
   </BOUNDS>
   <PIN pinname="Input String" slicecount="1" visible="0" values="connected">
   </PIN>
   <PIN pinname="Output String" visible="0">
   </PIN>
   <PIN pinname="Show Grid" slicecount="1" values="0">
   </PIN>
   </NODE>
   <LINK dstnodeid="5" dstpinname="Y Input Value" srcnodeid="7" srcpinname="Connected">
   </LINK>
   <LINK dstnodeid="6" dstpinname="Y Input Value" srcnodeid="7" srcpinname="Output">
   </LINK>
   <NODE componentmode="InABox" id="3" nodename="IOBox (Value Advanced)">
   <BOUNDS height="0" left="465" top="3120" type="Node" width="0">
   </BOUNDS>
   <BOUNDS height="160" left="7620" top="16545" type="Window" width="215">
   </BOUNDS>
   <BOUNDS height="300" left="465" top="3120" type="Box" width="3150">
   </BOUNDS>
   <PIN pinname="Show Value" slicecount="1" values="0">
   </PIN>
   <PIN pinname="Show Slider" slicecount="1" values="1">
   </PIN>
   <PIN pinname="Minimum" slicecount="1" values="0">
   </PIN>
   <PIN pinname="Maximum" slicecount="1" values="1">
   </PIN>
   <PIN pinname="Slider Behavior" slicecount="1" values="Toggle">
   </PIN>
   <PIN pinname="Y Input Value" visible="1">
   </PIN>
   <PIN pinname="Columns" slicecount="1" values="12">
   </PIN>
   <PIN pinname="SliceCount Mode" slicecount="1" values="ColsRowsPages">
   </PIN>
   <PIN pinname="Y Output Value" visible="1">
   </PIN>
   </NODE>
   <NODE componentmode="InABox" id="2" nodename="IOBox (String)">
   <BOUNDS height="270" left="1665" top="2805" type="Node" width="435">
   </BOUNDS>
   <BOUNDS height="270" left="1665" top="2805" type="Box" width="690">
   </BOUNDS>
   <BOUNDS height="160" left="0" top="0" type="Window" width="215">
   </BOUNDS>
   <PIN pinname="Input String" slicecount="1" visible="0" values="outputs">
   </PIN>
   <PIN pinname="Output String" visible="0">
   </PIN>
   <PIN pinname="Show Grid" slicecount="1" values="0">
   </PIN>
   </NODE>
   <NODE componentmode="InABox" id="1" nodename="IOBox (String)">
   <BOUNDS height="270" left="1710" top="4410" type="Node" width="330">
   </BOUNDS>
   <BOUNDS height="315" left="1710" top="4410" type="Box" width="570">
   </BOUNDS>
   <BOUNDS height="160" left="0" top="0" type="Window" width="215">
   </BOUNDS>
   <PIN pinname="Input String" slicecount="1" visible="0" values="inputs">
   </PIN>
   <PIN pinname="Output String" visible="0">
   </PIN>
   <PIN pinname="Show Grid" slicecount="1" values="0">
   </PIN>
   </NODE>
   <NODE id="16" nodename="LFO (Animation)">
   <BOUNDS height="0" left="3555" top="1335" type="Node" width="0">
   </BOUNDS>
   <PIN pinname="Output" visible="1">
   </PIN>
   <PIN pinname="Period" slicecount="1" values="2">
   </PIN>
   </NODE>
   <NODE id="15" nodename="MapRange (Value)">
   <BOUNDS height="0" left="3555" top="1680" type="Node" width="0">
   </BOUNDS>
   <PIN pinname="Input" visible="1">
   </PIN>
   <PIN pinname="Destination Center" slicecount="1" values="6">
   </PIN>
   <PIN pinname="Destination Width" slicecount="1" values="12">
   </PIN>
   <PIN pinname="Output" visible="1">
   </PIN>
   </NODE>
   <NODE id="14" nodename="Frac (Value)">
   <BOUNDS height="0" left="3555" top="2025" type="Node" width="0">
   </BOUNDS>
   <PIN pinname="Input" visible="1">
   </PIN>
   <PIN pinname="Whole Part" visible="1">
   </PIN>
   </NODE>
   <LINK dstnodeid="14" dstpinname="Input" srcnodeid="15" srcpinname="Output">
   </LINK>
   <LINK dstnodeid="15" dstpinname="Input" srcnodeid="16" srcpinname="Output">
   </LINK>
   <NODE nodename="EQ (Value)" id="17">
   <BOUNDS type="Node" left="3540" top="2715" width="0" height="0">
   </BOUNDS>
   <PIN pinname="Input 2" visible="1">
   </PIN>
   <PIN pinname="Input 1" visible="1">
   </PIN>
   <PIN pinname="Output" visible="1">
   </PIN>
   </NODE>
   <NODE nodename="I (Spreads)" id="18">
   <BOUNDS type="Node" left="3720" top="2370" width="0" height="0">
   </BOUNDS>
   <PIN pinname=".. To [" slicecount="1" values="12">
   </PIN>
   <PIN pinname="Output" visible="1">
   </PIN>
   </NODE>
   <LINK srcnodeid="18" srcpinname="Output" dstnodeid="17" dstpinname="Input 2">
   </LINK>
   <LINK srcnodeid="14" srcpinname="Whole Part" dstnodeid="17" dstpinname="Input 1">
   </LINK>
   <LINK srcnodeid="17" srcpinname="Output" dstnodeid="3" dstpinname="Y Input Value">
   </LINK>
   <LINK srcnodeid="3" srcpinname="Y Output Value" dstnodeid="7" dstpinname="Input">
   </LINK>
   <NODE nodename="IOBox (String)" componentmode="InABox" id="19">
   <BOUNDS type="Node" left="4800" top="3135" width="825" height="270">
   </BOUNDS>
   <BOUNDS type="Box" left="4800" top="3135" width="1170" height="270">
   </BOUNDS>
   <BOUNDS type="Window" left="0" top="0" width="215" height="160">
   </BOUNDS>
   <PIN pinname="Input String" visible="0" slicecount="1" values="192.168.1.1">
   </PIN>
   <PIN pinname="Output String" visible="1">
   </PIN>
   <PIN pinname="Show Grid" slicecount="1" values="0">
   </PIN>
   </NODE>
   <LINK srcnodeid="19" srcpinname="Output String" dstnodeid="7" dstpinname="IP Address">
   </LINK>
   <NODE componentmode="InABox" id="21" nodename="IOBox (String)">
   <BOUNDS height="270" left="7035" top="1290" type="Node" width="3960">
   </BOUNDS>
   <BOUNDS height="5640" left="7035" top="1290" type="Box" width="4875">
   </BOUNDS>
   <BOUNDS height="160" left="300" top="300" type="Window" width="215">
   </BOUNDS>
   <PIN pinname="Input String" slicecount="1" visible="0" values="|this node supports the newer W&amp;T Web-IO devices as well, but you need to change the configuration of the W&amp;T box to make it work: &cr;&lf;&cr;&lf;1. connect to the Web-IO device with a web browser&cr;&lf;2. click &apos;config&apos; and login as administrator in expert mode&cr;&lf;&cr;&lf;3. go to Config:Device:Basic Settings:Binary 1&cr;&lf;4. make sure  &apos;Enable BINARY 1&apos; is checked&cr;&lf;5. click the &apos;Temporary Storage&apos; button&cr;&lf;&cr;&lf;6. go to Config:Device:Basic Settings:Binary 1:TCP Server&cr;&lf;7. under Application Mode, select &apos;Compatible 50xxx&apos;&cr;&lf;8. click the &apos;Temporary Storage&apos; button&cr;&lf;&cr;&lf;9. go to Config:Device:Basic Settings:Output Mode&cr;&lf;10. select &apos;Binary 1&apos; for all outputs you want to control&cr;&lf;11. click the &apos;Temporary Storage&apos; button&cr;&lf;&cr;&lf;12. click on &apos;Logout&apos;&cr;&lf;13. click on &apos;Save&apos;&cr;&lf;&cr;&lf;now it should work! &cr;&lf;&cr;&lf;if the &apos;connected&apos; pin does not light up, check Renderer (TTY) to see what is going on. make sure you can ping the device, telnet to the port specified by the TCP Port pin, etc. |">
   </PIN>
   <PIN pinname="Output String" visible="0">
   </PIN>
   <PIN pinname="Show Grid" slicecount="1" values="0">
   </PIN>
   </NODE>
   <NODE nodename="IOBox (String)" componentmode="InABox" id="23">
   <BOUNDS type="Node" left="7065" top="735" width="375" height="270">
   </BOUNDS>
   <BOUNDS type="Box" left="7065" top="735" width="3675" height="360">
   </BOUNDS>
   <BOUNDS type="Window" left="0" top="0" width="215" height="160">
   </BOUNDS>
   <PIN pinname="Input String" visible="0" slicecount="1" values="|note for Web-IO devices only:|">
   </PIN>
   <PIN pinname="Output String" visible="0">
   </PIN>
   <PIN pinname="Show Grid" slicecount="1" values="0">
   </PIN>
   <PIN pinname="Size" slicecount="1" values="12">
   </PIN>
   </NODE>
   </PATCH>