<!DOCTYPE VVVV  SYSTEM "http://vvvv.meso.net/versions/vvvv33alpha7.8.dtd" >
   <PATCH nodename="C:\Dokumente und Einstellungen\AmpOp\Eigene Dateien\meso\dev\vvvv33\help\Boygroup (VVVV Server) help.v4p">
   <BOUNDS height="5790" left="2865" top="3375" type="Window" width="8955">
   </BOUNDS>
   <NODE componentmode="InABox" id="8" nodename="IOBox (String)">
   <PIN pinname="Show Grid" slicecount="1" values="0.00000">
   </PIN>
   <PIN pinname="Output String" visible="0">
   </PIN>
   <PIN pinname="Input String" slicecount="1" visible="0" values="|Clients: takes a spread if ip-addresses to specify which clients are welcome to join the boygroup setup|">
   </PIN>
   <BOUNDS height="160" left="0" top="0" type="Window" width="215">
   </BOUNDS>
   <BOUNDS height="705" left="420" top="1230" type="Box" width="2775">
   </BOUNDS>
   <BOUNDS height="255" left="420" top="1230" type="Node" width="1350">
   </BOUNDS>
   </NODE>
   <NODE componentmode="InABox" id="6" nodename="IOBox (Enumerations)">
   <BOUNDS height="0" left="4005" top="3015" type="Node" width="0">
   </BOUNDS>
   <BOUNDS height="160" left="6735" top="7650" type="Window" width="215">
   </BOUNDS>
   <BOUNDS height="270" left="4005" top="3015" type="Box" width="840">
   </BOUNDS>
   <PIN pinname="Output Enum" visible="1">
   </PIN>
   <PIN pinname="Input Enum" slicecount="1" values="UDP">
   </PIN>
   </NODE>
   <NODE componentmode="InABox" id="5" nodename="IOBox (Enumerations)">
   <BOUNDS height="0" left="3600" top="2625" type="Node" width="0">
   </BOUNDS>
   <BOUNDS height="160" left="7035" top="7950" type="Window" width="215">
   </BOUNDS>
   <BOUNDS height="255" left="3600" top="2625" type="Box" width="1275">
   </BOUNDS>
   <PIN pinname="Output Enum" visible="1">
   </PIN>
   <PIN pinname="Input Enum" slicecount="1" values="Connection">
   </PIN>
   </NODE>
   <NODE componentmode="InABox" id="4" nodename="IOBox (String)">
   <PIN pinname="Show Grid" slicecount="1" values="0.00000">
   </PIN>
   <PIN pinname="Output String" visible="0">
   </PIN>
   <PIN pinname="Input String" slicecount="1" visible="0" values="|Connected: &cr;&lf;a spread of  0 and 1 related to the Clients input spread showing the connection status.|">
   </PIN>
   <BOUNDS height="160" left="300" top="300" type="Window" width="215">
   </BOUNDS>
   <BOUNDS height="915" left="15" top="4185" type="Box" width="2415">
   </BOUNDS>
   <BOUNDS height="255" left="15" top="4185" type="Node" width="1350">
   </BOUNDS>
   </NODE>
   <NODE componentmode="InABox" id="3" nodename="IOBox (String)">
   <PIN pinname="Show Grid" slicecount="1" values="0.00000">
   </PIN>
   <PIN pinname="Output String" visible="0">
   </PIN>
   <PIN pinname="Input String" slicecount="1" visible="0" values="|Log to TTY: defines the loglevel for the messages written to the TTY-renderer|">
   </PIN>
   <BOUNDS height="160" left="300" top="300" type="Window" width="215">
   </BOUNDS>
   <BOUNDS height="525" left="3600" top="2085" type="Box" width="2940">
   </BOUNDS>
   <BOUNDS height="255" left="3600" top="2085" type="Node" width="1350">
   </BOUNDS>
   </NODE>
   <NODE componentmode="InABox" id="2" nodename="IOBox (String)">
   <PIN pinname="Show Grid" slicecount="1" values="0.00000">
   </PIN>
   <PIN pinname="Output String" visible="0">
   </PIN>
   <PIN pinname="Input String" slicecount="1" visible="0" values="|BroadcastMode:&cr;&lf;+ UDP: boygroup messages will be transmitted via UDP broadcast, graph related messages will still be transmitted via TCP. use this mode as default.&cr;&lf;+ TCP: all boygroup messages will be transmitted via TCP. no need for you to use this  mode.&cr;&lf;+ Quiet: no value updates will be transmitted|">
   </PIN>
   <BOUNDS height="160" left="600" top="600" type="Window" width="215">
   </BOUNDS>
   <BOUNDS height="1560" left="4875" top="3015" type="Box" width="3735">
   </BOUNDS>
   <BOUNDS height="255" left="4875" top="3015" type="Node" width="1350">
   </BOUNDS>
   </NODE>
   <NODE id="-5" nodename="Boygroup (VVVV Server)">
   <BOUNDS height="0" left="3225" top="3645" type="Node" width="0">
   </BOUNDS>
   <PIN pinname="Clients" visible="1">
   </PIN>
   <PIN pinname="Log to TTY" visible="1">
   </PIN>
   <PIN pinname="Broadcast Mode" visible="1">
   </PIN>
   <PIN pinname="Connected" visible="1">
   </PIN>
   </NODE>
   <NODE componentmode="InABox" id="1" nodename="IOBox (String)">
   <BOUNDS height="0" left="3225" top="1215" type="Node" width="0">
   </BOUNDS>
   <BOUNDS height="160" left="8835" top="6585" type="Window" width="215">
   </BOUNDS>
   <BOUNDS height="750" left="3225" top="1215" type="Box" width="1215">
   </BOUNDS>
   <PIN pinname="Rows" slicecount="1" values="3.00000">
   </PIN>
   <PIN pinname="Show Grid" slicecount="1" values="1.00000">
   </PIN>
   <PIN pinname="Input String" slicecount="3" values="192.168.0.2,192.168.0.3,192.168.0.4">
   </PIN>
   <PIN pinname="Output String" visible="1">
   </PIN>
   </NODE>
   <LINK dstnodeid="-5" dstpinname="Clients" srcnodeid="1" srcpinname="Output String">
   </LINK>
   <LINK dstnodeid="-5" dstpinname="Log to TTY" srcnodeid="5" srcpinname="Output Enum">
   </LINK>
   <LINK dstnodeid="-5" dstpinname="Broadcast Mode" srcnodeid="6" srcpinname="Output Enum">
   </LINK>
   <NODE componentmode="InABox" id="0" nodename="IOBox (Value Advanced)">
   <BOUNDS height="0" left="2475" top="4305" type="Node" width="0">
   </BOUNDS>
   <BOUNDS height="160" left="5640" top="8355" type="Window" width="215">
   </BOUNDS>
   <BOUNDS height="795" left="2475" top="4305" type="Box" width="810">
   </BOUNDS>
   <PIN pinname="Y Input Value" visible="1">
   </PIN>
   <PIN pinname="Rows" slicecount="1" values="3.00000">
   </PIN>
   <PIN pinname="Show Grid" slicecount="1" values="1.00000">
   </PIN>
   </NODE>
   <LINK dstnodeid="0" dstpinname="Y Input Value" srcnodeid="-5" srcpinname="Connected">
   </LINK>
   <NODE componentmode="InABox" id="10" nodename="IOBox (String)">
   <BOUNDS height="255" left="15" top="390" type="Node" width="570">
   </BOUNDS>
   <BOUNDS height="300" left="15" top="390" type="Box" width="3705">
   </BOUNDS>
   <BOUNDS height="160" left="510" top="7440" type="Window" width="215">
   </BOUNDS>
   <PIN pinname="Input String" slicecount="1" visible="0" values="|defines the render server in a multi-machine setup|">
   </PIN>
   <PIN pinname="Output String" visible="0">
   </PIN>
   <PIN pinname="Show Grid" slicecount="1" values="0.00000">
   </PIN>
   </NODE>
   <NODE componentmode="InABox" id="9" nodename="IOBox (String)">
   <BOUNDS height="270" left="15" top="15" type="Node" width="915">
   </BOUNDS>
   <BOUNDS height="390" left="15" top="15" type="Box" width="4095">
   </BOUNDS>
   <BOUNDS height="160" left="510" top="7440" type="Window" width="215">
   </BOUNDS>
   <PIN pinname="Input String" slicecount="1" visible="0" values="|Boygroup - VVVV Server|">
   </PIN>
   <PIN pinname="Output String" visible="0">
   </PIN>
   <PIN pinname="Show Grid" slicecount="1" values="0.00000">
   </PIN>
   <PIN pinname="Size" slicecount="1" values="12.00000">
   </PIN>
   </NODE>
   </PATCH>