<!DOCTYPE VVVV  SYSTEM "http://vvvv.meso.net/versions/vvvv33alpha7.8.dtd" >
   <PATCH nodename="C:\Dokumente und Einstellungen\AmpOp\Eigene Dateien\meso\dev\vvvv33\help\Delay (Animation) help.v4p">
   <BOUNDS height="7245" left="420" top="645" type="Window" width="12450">
   </BOUNDS>
   <NODE componentmode="InABox" id="13" nodename="IOBox (Value Advanced)">
   <BOUNDS height="0" left="1485" top="1740" type="Node" width="0">
   </BOUNDS>
   <BOUNDS height="160" left="7020" top="5250" type="Window" width="215">
   </BOUNDS>
   <BOUNDS height="1140" left="1485" top="1740" type="Box" width="780">
   </BOUNDS>
   <PIN pinname="Rows" slicecount="1" values="1.00000">
   </PIN>
   <PIN pinname="SliceCount Mode" slicecount="1" values="ColsRowsPages">
   </PIN>
   <PIN pinname="Y Input Value" slicecount="1" visible="1" values="0.56000">
   </PIN>
   <PIN pinname="Y Output Value" visible="1">
   </PIN>
   <PIN pinname="Show Grid" slicecount="1" values="1.00000">
   </PIN>
   <PIN pinname="Show Slider" slicecount="1" values="1.00000">
   </PIN>
   <PIN pinname="Minimum" slicecount="1" values="0.00000">
   </PIN>
   <PIN pinname="Maximum" slicecount="1" values="1.00000">
   </PIN>
   </NODE>
   <NODE componentmode="InABox" id="12" nodename="IOBox (Value Advanced)">
   <BOUNDS height="0" left="150" top="4350" type="Node" width="0">
   </BOUNDS>
   <BOUNDS height="160" left="7320" top="5550" type="Window" width="215">
   </BOUNDS>
   <BOUNDS height="2355" left="150" top="4350" type="Box" width="12030">
   </BOUNDS>
   <PIN pinname="Rows" slicecount="1" values="1.00000">
   </PIN>
   <PIN pinname="SliceCount Mode" slicecount="1" values="ColsRowsPages">
   </PIN>
   <PIN pinname="Y Input Value" slicecount="100" visible="1">
   </PIN>
   <PIN pinname="Y Output Value" visible="1">
   </PIN>
   <PIN pinname="Pages" slicecount="1" values="1.00000">
   </PIN>
   <PIN pinname="Columns" slicecount="1" values="100.00000">
   </PIN>
   <PIN pinname="Show Grid" slicecount="1" values="1.00000">
   </PIN>
   <PIN pinname="Show Slider" slicecount="1" values="1.00000">
   </PIN>
   <PIN pinname="Minimum" slicecount="1" values="0.00000">
   </PIN>
   <PIN pinname="Maximum" slicecount="1" values="1.00000">
   </PIN>
   </NODE>
   <NODE id="11" nodename="LinearSpread (Spreads)">
   <BOUNDS height="0" left="2400" top="2580" type="Node" width="0">
   </BOUNDS>
   <PIN pinname="Output" visible="1">
   </PIN>
   <PIN pinname="Width" slicecount="1" values="10.00000">
   </PIN>
   <PIN pinname="Input" slicecount="1" values="5.00000">
   </PIN>
   <PIN pinname="Alignment" slicecount="1" values="Block">
   </PIN>
   <PIN pinname="Spread Count" slicecount="1" values="100.00000">
   </PIN>
   </NODE>
   <NODE componentmode="InABox" id="10" nodename="IOBox (String)">
   <BOUNDS height="255" left="15" top="2940" type="Node" width="2070">
   </BOUNDS>
   <BOUNDS height="240" left="15" top="2940" type="Box" width="2205">
   </BOUNDS>
   <BOUNDS height="160" left="0" top="0" type="Window" width="215">
   </BOUNDS>
   <PIN pinname="Input String" slicecount="1" visible="0" values="|input of values to be delayed|">
   </PIN>
   <PIN pinname="Output String" visible="0">
   </PIN>
   <PIN pinname="Show Grid" slicecount="1" values="0.00000">
   </PIN>
   </NODE>
   <NODE componentmode="InABox" id="9" nodename="IOBox (String)">
   <BOUNDS height="255" left="2535" top="2940" type="Node" width="2205">
   </BOUNDS>
   <BOUNDS height="240" left="2535" top="2940" type="Box" width="2460">
   </BOUNDS>
   <BOUNDS height="160" left="0" top="0" type="Window" width="215">
   </BOUNDS>
   <PIN pinname="Input String" slicecount="1" visible="0" values="|input of delay-times in seconds|">
   </PIN>
   <PIN pinname="Output String" visible="0">
   </PIN>
   <PIN pinname="Show Grid" slicecount="1" values="0.00000">
   </PIN>
   </NODE>
   <NODE componentmode="InABox" id="8" nodename="IOBox (String)">
   <BOUNDS height="255" left="2880" top="3750" type="Node" width="2355">
   </BOUNDS>
   <BOUNDS height="285" left="2880" top="3750" type="Box" width="2820">
   </BOUNDS>
   <BOUNDS height="160" left="0" top="0" type="Window" width="215">
   </BOUNDS>
   <PIN pinname="Input String" slicecount="1" visible="0" values="|spread of delayed values returned|">
   </PIN>
   <PIN pinname="Output String" visible="0">
   </PIN>
   <PIN pinname="Show Grid" slicecount="1" values="0.00000">
   </PIN>
   </NODE>
   <NODE id="6" nodename="LFO (Animation)">
   <BOUNDS height="0" left="1890" top="765" type="Node" width="0">
   </BOUNDS>
   <PIN pinname="Output" visible="1">
   </PIN>
   <PIN pinname="Period" slicecount="1" values="20.00000">
   </PIN>
   <PIN pinname="Cycles" visible="1">
   </PIN>
   <PIN pinname="Reverse" slicecount="1" values="0.00000">
   </PIN>
   </NODE>
   <NODE id="5" nodename="Delay (Animation)">
   <BOUNDS height="0" left="2205" top="3735" type="Node" width="0">
   </BOUNDS>
   <PIN pinname="Input" visible="1">
   </PIN>
   <PIN pinname="Time" visible="1">
   </PIN>
   <PIN pinname="Output" visible="1">
   </PIN>
   <PIN pinname="Mode" slicecount="1" visible="1" values="Linear">
   </PIN>
   </NODE>
   <LINK dstnodeid="5" dstpinname="Input" srcnodeid="13" srcpinname="Y Output Value">
   </LINK>
   <LINK dstnodeid="5" dstpinname="Time" srcnodeid="11" srcpinname="Output">
   </LINK>
   <LINK dstnodeid="12" dstpinname="Y Input Value" srcnodeid="5" srcpinname="Output" linkstyle="VHV">
   <LINKPOINT x="2235" y="4215">
   </LINKPOINT>
   <LINKPOINT x="15480" y="4215">
   </LINKPOINT>
   </LINK>
   <NODE id="4" nodename="TypoSpread (Spreads)">
   <BOUNDS height="0" left="765" top="1200" type="Node" width="0">
   </BOUNDS>
   <PIN pinname="Input X" slicecount="1" visible="1" values="0.50000">
   </PIN>
   <PIN pinname="Output X" visible="1">
   </PIN>
   <PIN pinname="Phase" visible="1">
   </PIN>
   <PIN pinname="Text" slicecount="1" values="8">
   </PIN>
   <PIN pinname="Output Y" visible="1">
   </PIN>
   <PIN pinname="Input Y" slicecount="1" values="0.50000">
   </PIN>
   </NODE>
   <LINK dstnodeid="4" dstpinname="Phase" srcnodeid="6" srcpinname="Output">
   </LINK>
   <LINK dstnodeid="13" dstpinname="Y Input Value" srcnodeid="4" srcpinname="Output Y">
   </LINK>
   <NODE componentmode="InABox" id="3" nodename="IOBox (String)">
   <BOUNDS height="255" left="3780" top="3360" type="Node" width="2520">
   </BOUNDS>
   <BOUNDS height="315" left="3780" top="3360" type="Box" width="3285">
   </BOUNDS>
   <BOUNDS height="160" left="0" top="0" type="Window" width="215">
   </BOUNDS>
   <PIN pinname="Input String" slicecount="1" visible="0" values="|linear mode will interpolate between samples|">
   </PIN>
   <PIN pinname="Output String" visible="0">
   </PIN>
   <PIN pinname="Show Grid" slicecount="1" values="0.00000">
   </PIN>
   </NODE>
   <NODE componentmode="InABox" id="1" nodename="IOBox (String)">
   <BOUNDS height="255" left="3465" top="2565" type="Node" width="2235">
   </BOUNDS>
   <BOUNDS height="300" left="3465" top="2565" type="Box" width="2685">
   </BOUNDS>
   <BOUNDS height="160" left="0" top="0" type="Window" width="215">
   </BOUNDS>
   <PIN pinname="Input String" slicecount="1" visible="0" values="|create a spread with delay times|">
   </PIN>
   <PIN pinname="Output String" visible="0">
   </PIN>
   <PIN pinname="Show Grid" slicecount="1" values="0.00000">
   </PIN>
   </NODE>
   <NODE componentmode="InABox" id="0" nodename="IOBox (String)">
   <BOUNDS height="585" left="7035" top="60" type="Node" width="4635">
   </BOUNDS>
   <BOUNDS height="915" left="7035" top="60" type="Box" width="5250">
   </BOUNDS>
   <BOUNDS height="160" left="0" top="0" type="Window" width="215">
   </BOUNDS>
   <PIN pinname="Input String" slicecount="1" visible="0" values="|note that the delay node will store only the value of the last 1024 frames.&cr;&lf; &cr;&lf;the actual time you can delay therefore is related to your frame rate.&cr;&lf;for example if you are running at 20fps you can delay up to 50 seconds|">
   </PIN>
   <PIN pinname="Output String" visible="0">
   </PIN>
   <PIN pinname="Show Grid" slicecount="1" values="0.00000">
   </PIN>
   </NODE>
   <NODE componentmode="InABox" id="15" nodename="IOBox (String)">
   <BOUNDS height="255" left="15" top="390" type="Node" width="570">
   </BOUNDS>
   <BOUNDS height="315" left="15" top="390" type="Box" width="3060">
   </BOUNDS>
   <BOUNDS height="160" left="-450" top="2010" type="Window" width="215">
   </BOUNDS>
   <PIN pinname="Input String" slicecount="1" visible="0" values="|Delays incoming values for a certain time&cr;&lf;|">
   </PIN>
   <PIN pinname="Output String" visible="0">
   </PIN>
   <PIN pinname="Show Grid" slicecount="1" values="0.00000">
   </PIN>
   </NODE>
   <NODE componentmode="InABox" id="14" nodename="IOBox (String)">
   <BOUNDS height="270" left="15" top="15" type="Node" width="915">
   </BOUNDS>
   <BOUNDS height="390" left="15" top="15" type="Box" width="4095">
   </BOUNDS>
   <BOUNDS height="160" left="150" top="2610" type="Window" width="215">
   </BOUNDS>
   <PIN pinname="Input String" slicecount="1" visible="0" values="|Delay - Animation|">
   </PIN>
   <PIN pinname="Output String" visible="0">
   </PIN>
   <PIN pinname="Show Grid" slicecount="1" values="0.00000">
   </PIN>
   <PIN pinname="Size" slicecount="1" values="12.00000">
   </PIN>
   </NODE>
   <NODE nodename="IOBox (Enumerations)" componentmode="InABox" id="16">
   <BOUNDS type="Node" left="2745" top="3375" width="0" height="0">
   </BOUNDS>
   <BOUNDS type="Window" left="7530" top="5250" width="215" height="160">
   </BOUNDS>
   <BOUNDS type="Box" left="2745" top="3375" width="1005" height="240">
   </BOUNDS>
   <PIN pinname="Output Enum" visible="1">
   </PIN>
   </NODE>
   <LINK srcnodeid="16" srcpinname="Output Enum" dstnodeid="5" dstpinname="Mode">
   </LINK>
   </PATCH>