<!DOCTYPE VVVV  SYSTEM "http://vvvv.meso.net/versions/vvvv33alpha7.8.dtd" >
   <PATCH componentmode="InAWindow" nodename="C:\Dokumente und Einstellungen\AmpOp\Eigene Dateien\meso\dev\vvvv33\help\Boost (VVVV) help.v4p">
   <BOUNDS height="5310" left="1320" top="2895" type="Window" width="7425">
   </BOUNDS>
   <NODE id="-5" nodename="Boost (VVVV)">
   <BOUNDS height="0" left="645" top="3060" type="Node" width="0">
   </BOUNDS>
   <PIN pinname="Enabled" visible="1">
   </PIN>
   </NODE>
   <NODE componentmode="InABox" id="0" nodename="IOBox (String)">
   <BOUNDS height="420" left="1455" top="1320" type="Node" width="3330">
   </BOUNDS>
   <BOUNDS height="3480" left="1455" top="1320" type="Box" width="5715">
   </BOUNDS>
   <BOUNDS height="160" left="0" top="0" type="Window" width="215">
   </BOUNDS>
   <PIN pinname="Input String" slicecount="1" visible="0" values="|Note: Experimental Feature to get maximum performance during rendering&cr;&lf;&cr;&lf;if enabled = 1&cr;&lf;sets the application priority to HIGH and the main threads priority to HIGHEST&cr;&lf;&cr;&lf;id enabled = 0&cr;&lf;sets the application priority to NORMAL.&cr;&lf;&cr;&lf;if enabled = -1&cr;&lf;sets the application priority to LOW.&cr;&lf;&cr;&lf;The threads of the process preempt the threads of normal or idle priority class processes.  Use extreme care when using the high-priority class, because a high-priority class application can use nearly all available CPU time.&cr;&lf;&cr;&lf;You may need to have Administrator rights on your machine to use this node.|">
   </PIN>
   <PIN pinname="Output String" visible="0">
   </PIN>
   <PIN pinname="Show Grid" slicecount="1" values="0.00000">
   </PIN>
   </NODE>
   <NODE componentmode="InABox" id="2" nodename="IOBox (String)">
   <BOUNDS height="255" left="15" top="390" type="Node" width="570">
   </BOUNDS>
   <BOUNDS height="495" left="15" top="390" type="Box" width="4725">
   </BOUNDS>
   <BOUNDS height="160" left="510" top="5190" type="Window" width="215">
   </BOUNDS>
   <PIN pinname="Input String" slicecount="1" visible="0" values="|Sets vvvv´s priority in the systems. On NT systems you must have PROCESS_SET_INFORMATION rights to set the priority|">
   </PIN>
   <PIN pinname="Output String" visible="0">
   </PIN>
   <PIN pinname="Show Grid" slicecount="1" values="0.00000">
   </PIN>
   </NODE>
   <NODE componentmode="InABox" id="1" nodename="IOBox (String)">
   <BOUNDS height="270" left="15" top="15" type="Node" width="915">
   </BOUNDS>
   <BOUNDS height="375" left="15" top="15" type="Box" width="4320">
   </BOUNDS>
   <BOUNDS height="160" left="510" top="5190" type="Window" width="215">
   </BOUNDS>
   <PIN pinname="Input String" slicecount="1" visible="0" values="|Boost - VVVV|">
   </PIN>
   <PIN pinname="Output String" visible="0">
   </PIN>
   <PIN pinname="Show Grid" slicecount="1" values="0.00000">
   </PIN>
   <PIN pinname="Size" slicecount="1" values="12.00000">
   </PIN>
   </NODE>
   <NODE nodename="IOBox (Value Advanced)" componentmode="InABox" id="7">
   <BOUNDS type="Node" left="240" top="2415" width="0" height="0">
   </BOUNDS>
   <BOUNDS type="Window" left="2145" top="5430" width="215" height="160">
   </BOUNDS>
   <BOUNDS type="Box" left="240" top="2415" width="450" height="360">
   </BOUNDS>
   <PIN pinname="Y Input Value" visible="1" slicecount="1" values="-1.00000">
   </PIN>
   <PIN pinname="Y Output Value" visible="1">
   </PIN>
   <PIN pinname="Minimum" slicecount="1" values="-1.00000">
   </PIN>
   <PIN pinname="Maximum" slicecount="1" values="1.00000">
   </PIN>
   <PIN pinname="Size" slicecount="1" values="12.00000">
   </PIN>
   </NODE>
   <LINK srcnodeid="7" srcpinname="Y Output Value" dstnodeid="-5" dstpinname="Enabled">
   </LINK>
   </PATCH>