<!DOCTYPE VVVV  SYSTEM "http://vvvv.meso.net/versions/vvvv33beta7.4.dtd" >
   <PATCH nodename="X:\vvvv33\help\NetSend (Network Value) help.v4p">
   <BOUNDS height="4515" left="480" top="975" type="Window" width="6570">
   </BOUNDS>
   <NODE componentmode="InABox" id="8" nodename="IOBox (Value Advanced)">
   <BOUNDS height="0" left="330" top="1695" type="Node" width="0">
   </BOUNDS>
   <BOUNDS height="160" left="7464" top="5325" type="Window" width="215">
   </BOUNDS>
   <BOUNDS height="285" left="330" top="1695" type="Box" width="750">
   </BOUNDS>
   <PIN pinname="Y Output Value" visible="1">
   </PIN>
   <PIN pinname="Y Input Value" slicecount="1" visible="1" values="0.63000">
   </PIN>
   </NODE>
   <NODE componentmode="InABox" id="7" nodename="IOBox (String)">
   <BOUNDS height="420" left="300" top="330" type="Node" width="1125">
   </BOUNDS>
   <BOUNDS height="555" left="300" top="330" type="Box" width="4185">
   </BOUNDS>
   <BOUNDS height="160" left="0" top="0" type="Window" width="215">
   </BOUNDS>
   <PIN pinname="Input String" slicecount="1" visible="0" values="|NetSend &cr;&lf;Sends values via UDP or TCP using PD&apos;s FUDI-protocol|">
   </PIN>
   <PIN pinname="Output String" visible="0">
   </PIN>
   <PIN pinname="Show Grid" slicecount="1" values="0.00000">
   </PIN>
   </NODE>
   <NODE componentmode="InABox" id="6" nodename="IOBox (String)">
   <BOUNDS height="255" left="2370" top="3000" type="Node" width="825">
   </BOUNDS>
   <BOUNDS height="255" left="2370" top="3000" type="Box" width="825">
   </BOUNDS>
   <BOUNDS height="160" left="0" top="0" type="Window" width="215">
   </BOUNDS>
   <PIN pinname="Input String" slicecount="1" visible="0" values="|see also|">
   </PIN>
   <PIN pinname="Output String" visible="0">
   </PIN>
   <PIN pinname="Show Grid" slicecount="1" values="0.00000">
   </PIN>
   </NODE>
   <NODE componentmode="InABox" id="5" nodename="IOBox (String)">
   <BOUNDS height="585" left="2370" top="1155" type="Node" width="3600">
   </BOUNDS>
   <BOUNDS height="960" left="2370" top="1155" type="Box" width="3930">
   </BOUNDS>
   <BOUNDS height="160" left="0" top="0" type="Window" width="215">
   </BOUNDS>
   <PIN pinname="Input String" slicecount="1" visible="0" values="|Based on the client socket nodes this module works like [netsend] known from pd. &cr;&lf;Choose a protocol, host and port to connect to. Sending a spread will be received as list in pd.|">
   </PIN>
   <PIN pinname="Output String" visible="0">
   </PIN>
   <PIN pinname="Show Grid" slicecount="1" values="0.00000">
   </PIN>
   </NODE>
   <NODE componentmode="InABox" id="4" nodename="IOBox (String)">
   <BOUNDS height="255" left="2370" top="2325" type="Node" width="4440">
   </BOUNDS>
   <BOUNDS height="525" left="2370" top="2325" type="Box" width="3360">
   </BOUNDS>
   <BOUNDS height="160" left="0" top="0" type="Window" width="215">
   </BOUNDS>
   <PIN pinname="Input String" slicecount="1" visible="0" values="|Open the help patch for NetReceive to see the nodes communicate|">
   </PIN>
   <PIN pinname="Output String" visible="0">
   </PIN>
   <PIN pinname="Show Grid" slicecount="1" values="0.00000">
   </PIN>
   </NODE>
   <NODE id="3" nodename="LFO (Animation)">
   <BOUNDS height="0" left="1020" top="1155" type="Node" width="0">
   </BOUNDS>
   <PIN pinname="Output" visible="1">
   </PIN>
   </NODE>
   <LINK dstnodeid="8" dstpinname="Y Input Value" srcnodeid="3" srcpinname="Output">
   </LINK>
   <NODE componentmode="InABox" id="2" nodename="IOBox (Value Advanced)">
   <BOUNDS height="0" left="615" top="2715" type="Node" width="0">
   </BOUNDS>
   <BOUNDS height="160" left="8064" top="5925" type="Window" width="215">
   </BOUNDS>
   <BOUNDS height="405" left="615" top="2715" type="Box" width="450">
   </BOUNDS>
   <PIN pinname="Y Output Value" visible="1">
   </PIN>
   <PIN pinname="Show Grid" slicecount="1" values="0.00000">
   </PIN>
   <PIN pinname="Show Slider" slicecount="1" values="1.00000">
   </PIN>
   <PIN pinname="Show Value" slicecount="1" values="0.00000">
   </PIN>
   <PIN pinname="Slider Behavior" slicecount="1" values="Toggle">
   </PIN>
   <PIN pinname="X Input Value" slicecount="1" values="1.00000">
   </PIN>
   <PIN pinname="Y Input Value" slicecount="1" visible="1">
   </PIN>
   <PIN pinname="Maximum" slicecount="1" values="1.00000">
   </PIN>
   <PIN pinname="Minimum" slicecount="1" values="0.00000">
   </PIN>
   </NODE>
   <NODE componentmode="Hidden" id="9" nodename=":MODULES:\Netsend (Network Value).v4p">
   <BOUNDS height="100" left="1020" top="2235" type="Node" width="100">
   </BOUNDS>
   <PIN pinname="Values" visible="1">
   </PIN>
   <PIN pinname="Connect" slicecount="1" values="1.00000">
   </PIN>
   <PIN pinname="Connected" visible="1">
   </PIN>
   <BOUNDS left="1020" top="2235" type="Box">
   </BOUNDS>
   <PIN pinname="Host" slicecount="1" values="127.0.0.1">
   </PIN>
   <PIN pinname="Protocol" slicecount="1" values="1.00000">
   </PIN>
   </NODE>
   <LINK dstnodeid="9" dstpinname="Values" srcnodeid="8" srcpinname="Y Output Value">
   </LINK>
   <LINK dstnodeid="2" dstpinname="Y Input Value" srcnodeid="9" srcpinname="Connected">
   </LINK>
   <NODE componentmode="Hidden" id="10" nodename=":MODULES:\Netreceive (Network Value).v4p">
   <BOUNDS height="100" left="2370" top="3330" type="Node" width="100">
   </BOUNDS>
   <BOUNDS left="2370" top="3330" type="Box">
   </BOUNDS>
   <PIN pinname="Connection Count" visible="1">
   </PIN>
   <PIN pinname="Values" visible="1">
   </PIN>
   <PIN pinname="Port" slicecount="1" values="4446.00000">
   </PIN>
   <BOUNDS height="9000" left="7155" top="1950" type="Window" width="9240">
   </BOUNDS>
   </NODE>
   </PATCH>