<!DOCTYPE PATCH  SYSTEM "http://vvvv.org/versions/vvvv33beta11.2.dtd" >
   <PATCH nodename="Y:\vvvv33_trunk\help\QRCodeTexture (EX9.Texture) help.v4p">
   <BOUNDS height="8745" left="13440" top="2295" type="Window" width="13215">
   </BOUNDS>
   <NODE id="17" nodename="LFO (Animation)">
   <BOUNDS height="270" left="5850" top="2625" type="Node" width="855">
   </BOUNDS>
   <PIN pinname="Cycles" visible="1">
   </PIN>
   <PIN pinname="Period" slicecount="1" values="1">
   </PIN>
   <PIN pinname="Phase" slicecount="1" values="0">
   </PIN>
   <PIN pinname="Reset" slicecount="1" values="0">
   </PIN>
   </NODE>
   <NODE id="16" nodename="SpellValue (String)">
   <BOUNDS height="0" left="5850" top="3075" type="Node" width="0">
   </BOUNDS>
   <PIN pinname="Input" visible="1">
   </PIN>
   <PIN pinname="Output" visible="1">
   </PIN>
   </NODE>
   <LINK dstnodeid="16" dstpinname="Input" srcnodeid="17" srcpinname="Cycles">
   </LINK>
   <NODE id="15" nodename="Quad (DX9)">
   <BOUNDS height="0" left="2925" top="7365" type="Node" width="0">
   </BOUNDS>
   <PIN pinname="Layer" visible="1">
   </PIN>
   <PIN pinname="Texture" visible="1">
   </PIN>
   <PIN pinname="Sampler State" slicecount="1" visible="1" values="||">
   </PIN>
   </NODE>
   <NODE componentmode="InABox" id="14" nodename="Renderer (EX9)">
   <BOUNDS height="270" left="8190" top="240" type="Node" width="3660">
   </BOUNDS>
   <BOUNDS height="6360" left="23010" top="15240" type="Window" width="6120">
   </BOUNDS>
   <BOUNDS height="4650" left="8190" top="240" type="Box" width="4530">
   </BOUNDS>
   <PIN pinname="Layers" visible="1">
   </PIN>
   <PIN pinname="Projection Transform" slicecount="1" visible="1" values="||">
   </PIN>
   <PIN pinname="Device" slicecount="1" values="-1">
   </PIN>
   </NODE>
   <NODE componentmode="InABox" id="13" nodename="IOBox (Value Advanced)">
   <BOUNDS height="0" left="7155" top="6990" type="Node" width="0">
   </BOUNDS>
   <BOUNDS height="160" left="19125" top="11745" type="Window" width="215">
   </BOUNDS>
   <BOUNDS height="240" left="7155" top="6990" type="Box" width="1020">
   </BOUNDS>
   <PIN pinname="Y Input Value" visible="1">
   </PIN>
   <PIN pinname="Descriptive Name" slicecount="1" values="|used version|">
   </PIN>
   </NODE>
   <NODE componentmode="InABox" id="12" nodename="IOBox (String)">
   <BOUNDS height="0" left="240" top="1620" type="Node" width="0">
   </BOUNDS>
   <BOUNDS height="160" left="19680" top="20010" type="Window" width="215">
   </BOUNDS>
   <BOUNDS height="1155" left="240" top="1620" type="Box" width="2235">
   </BOUNDS>
   <PIN pinname="Input String" slicecount="1" values="|BEGIN:VCARD&cr;&lf;N:Some name&cr;&lf;TEL:0123456789&cr;&lf;EMAIL:bla@bla.de&cr;&lf;END:VCARD|">
   </PIN>
   <PIN pinname="Output String" visible="1">
   </PIN>
   <PIN pinname="Descriptive Name" slicecount="1" values="|adress book entry|">
   </PIN>
   </NODE>
   <NODE componentmode="InABox" id="11" nodename="IOBox (String)">
   <BOUNDS height="0" left="2595" top="1620" type="Node" width="0">
   </BOUNDS>
   <BOUNDS height="160" left="17205" top="19425" type="Window" width="215">
   </BOUNDS>
   <BOUNDS height="510" left="2595" top="1620" type="Box" width="2280">
   </BOUNDS>
   <PIN pinname="Input String" slicecount="1" values="|SMSTO:0123456789:Hello QR-Code|">
   </PIN>
   <PIN pinname="Descriptive Name" slicecount="1" values="|prepared SMS|">
   </PIN>
   <PIN pinname="Output String" visible="1">
   </PIN>
   </NODE>
   <NODE componentmode="InABox" id="10" nodename="IOBox (String)">
   <BOUNDS height="0" left="4950" top="1620" type="Node" width="0">
   </BOUNDS>
   <BOUNDS height="160" left="20070" top="20640" type="Window" width="215">
   </BOUNDS>
   <BOUNDS height="255" left="4950" top="1620" type="Box" width="2400">
   </BOUNDS>
   <PIN pinname="Input String" slicecount="1" values="URL:http://www.meso.net">
   </PIN>
   <PIN pinname="Output String" visible="1">
   </PIN>
   <PIN pinname="Descriptive Name" slicecount="1" values="link">
   </PIN>
   </NODE>
   <NODE componentmode="InABox" id="9" nodename="IOBox (String)">
   <BOUNDS height="0" left="5475" top="1995" type="Node" width="0">
   </BOUNDS>
   <BOUNDS height="160" left="23010" top="21090" type="Window" width="215">
   </BOUNDS>
   <BOUNDS height="240" left="5475" top="1995" type="Box" width="1875">
   </BOUNDS>
   <PIN pinname="Input String" slicecount="1" values="TEL:0123456789">
   </PIN>
   <PIN pinname="Output String" visible="1">
   </PIN>
   <PIN pinname="Descriptive Name" slicecount="1" values="|predialed phone number|">
   </PIN>
   </NODE>
   <NODE componentmode="InABox" id="8" nodename="IOBox (String)">
   <BOUNDS height="270" left="165" top="540" type="Node" width="8220">
   </BOUNDS>
   <BOUNDS height="780" left="165" top="540" type="Box" width="4710">
   </BOUNDS>
   <BOUNDS height="160" left="300" top="300" type="Window" width="215">
   </BOUNDS>
   <PIN pinname="Input String" slicecount="1" visible="0" values="|QR-Code is a 2D-Barcode that can be decoded by cellular phones equipped with decoder software. Especially in Japan a huge number of phones is already shipped with a java decoder.|">
   </PIN>
   <PIN pinname="Output String" visible="0">
   </PIN>
   <PIN pinname="Show Grid" slicecount="1" values="0">
   </PIN>
   </NODE>
   <NODE componentmode="InABox" id="7" nodename="IOBox (String)">
   <BOUNDS height="270" left="165" top="165" type="Node" width="915">
   </BOUNDS>
   <BOUNDS height="375" left="165" top="165" type="Box" width="4740">
   </BOUNDS>
   <BOUNDS height="160" left="7950" top="5220" type="Window" width="215">
   </BOUNDS>
   <PIN pinname="Input String" slicecount="1" visible="0" values="|QRCodeTexture - EX9.Texture|">
   </PIN>
   <PIN pinname="Output String" visible="0">
   </PIN>
   <PIN pinname="Show Grid" slicecount="1" values="0">
   </PIN>
   <PIN pinname="Size" slicecount="1" values="12">
   </PIN>
   </NODE>
   <LINK dstnodeid="14" dstpinname="Layers" srcnodeid="15" srcpinname="Layer">
   <LINKPOINT x="2955" y="8040">
   </LINKPOINT>
   <LINKPOINT x="7710" y="8040">
   </LINKPOINT>
   <LINKPOINT x="7710" y="255">
   </LINKPOINT>
   </LINK>
   <NODE componentmode="InABox" id="6" nodename="IOBox (String)">
   <BOUNDS height="270" left="15" top="3570" type="Node" width="3180">
   </BOUNDS>
   <BOUNDS height="540" left="15" top="3570" type="Box" width="2130">
   </BOUNDS>
   <BOUNDS height="160" left="0" top="0" type="Window" width="215">
   </BOUNDS>
   <PIN pinname="Input String" slicecount="1" visible="0" values="|Try different special features for cellular phones -&gt;|">
   </PIN>
   <PIN pinname="Output String" visible="0">
   </PIN>
   <PIN pinname="Show Grid" slicecount="1" values="0">
   </PIN>
   </NODE>
   <NODE componentmode="InABox" id="5" nodename="IOBox (String)">
   <BOUNDS height="270" left="8280" top="6015" type="Node" width="3930">
   </BOUNDS>
   <BOUNDS height="1395" left="8280" top="6015" type="Box" width="4350">
   </BOUNDS>
   <BOUNDS height="160" left="0" top="0" type="Window" width="215">
   </BOUNDS>
   <PIN pinname="Input String" slicecount="1" visible="0" values="|See the following link if you want to know about QR-Code details such as &apos;version&apos;&cr;&lf;http://www.denso-wave.com/qrcode/qrgene2-e.html&cr;&lf;&cr;&lf;Versions above 10 are not guaranteed to be decoded by cellular phone software.|">
   </PIN>
   <PIN pinname="Output String" visible="0">
   </PIN>
   <PIN pinname="Show Grid" slicecount="1" values="0">
   </PIN>
   </NODE>
   <NODE id="4" nodename="QRCodeTexture (EX9.Texture)">
   <BOUNDS height="0" left="3240" top="6780" type="Node" width="0">
   </BOUNDS>
   <PIN pinname="Text" visible="1">
   </PIN>
   <PIN pinname="DataDirectory" visible="1">
   </PIN>
   </NODE>
   <LINK dstnodeid="15" dstpinname="Texture" srcnodeid="4" srcpinname="Texture Out">
   </LINK>
   <LINK dstnodeid="13" dstpinname="Y Input Value" srcnodeid="4" srcpinname="Version">
   </LINK>
   <NODE id="3" nodename="Switch (String Input)">
   <BOUNDS height="0" left="3240" top="4050" type="Node" width="0">
   </BOUNDS>
   <PIN pinname="Input Count" slicecount="1" values="5">
   </PIN>
   <PIN pinname="Input 1" visible="1">
   </PIN>
   <PIN pinname="Input 2" visible="1">
   </PIN>
   <PIN pinname="Input 3" visible="1">
   </PIN>
   <PIN pinname="Input 4" visible="1">
   </PIN>
   <PIN pinname="Input 5" visible="1">
   </PIN>
   <PIN pinname="Output" visible="1">
   </PIN>
   <PIN pinname="Switch" visible="1">
   </PIN>
   </NODE>
   <LINK dstnodeid="3" dstpinname="Input 1" srcnodeid="12" srcpinname="Output String">
   </LINK>
   <LINK dstnodeid="3" dstpinname="Input 2" srcnodeid="11" srcpinname="Output String">
   </LINK>
   <LINK dstnodeid="3" dstpinname="Input 3" srcnodeid="10" srcpinname="Output String">
   </LINK>
   <LINK dstnodeid="3" dstpinname="Input 4" srcnodeid="9" srcpinname="Output String">
   </LINK>
   <LINK dstnodeid="3" dstpinname="Input 5" srcnodeid="16" srcpinname="Output">
   </LINK>
   <LINK dstnodeid="4" dstpinname="Text" srcnodeid="3" srcpinname="Output">
   </LINK>
   <NODE componentmode="InABox" id="2" nodename="IOBox (Value Advanced)">
   <BOUNDS height="0" left="2205" top="3855" type="Node" width="0">
   </BOUNDS>
   <BOUNDS height="160" left="15225" top="6315" type="Window" width="215">
   </BOUNDS>
   <BOUNDS height="240" left="2205" top="3855" type="Box" width="450">
   </BOUNDS>
   <PIN pinname="Y Output Value" visible="1">
   </PIN>
   <PIN pinname="Y Input Value" slicecount="1" values="0">
   </PIN>
   </NODE>
   <LINK dstnodeid="3" dstpinname="Switch" srcnodeid="2" srcpinname="Y Output Value">
   </LINK>
   <NODE componentmode="InABox" id="1" nodename="IOBox (String)">
   <BOUNDS height="0" left="4410" top="6090" type="Node" width="0">
   </BOUNDS>
   <BOUNDS height="160" left="19815" top="8250" type="Window" width="215">
   </BOUNDS>
   <BOUNDS height="285" left="4410" top="6090" type="Box" width="1590">
   </BOUNDS>
   <PIN pinname="Output String" visible="1">
   </PIN>
   <PIN pinname="Input String" slicecount="1" values="..\bin\qrcode_data">
   </PIN>
   </NODE>
   <LINK dstnodeid="4" dstpinname="DataDirectory" srcnodeid="1" srcpinname="Output String">
   </LINK>
   <NODE componentmode="InABox" id="0" nodename="IOBox (String)">
   <BOUNDS height="270" left="3585" top="4920" type="Node" width="6285">
   </BOUNDS>
   <BOUNDS height="1125" left="3585" top="4920" type="Box" width="3855">
   </BOUNDS>
   <BOUNDS height="160" left="0" top="0" type="Window" width="215">
   </BOUNDS>
   <PIN pinname="Input String" slicecount="1" visible="0" values="|some binary data necessary for this node to work is available as a separate download from vvvv.org: &cr;&lf;http://vvvv.org/tiki-download_file.php?fileId=1407&cr;&lf;unpack the data to disk and choose the directory here:|">
   </PIN>
   <PIN pinname="Output String" visible="0">
   </PIN>
   <PIN pinname="Show Grid" slicecount="1" values="0">
   </PIN>
   </NODE>
   </PATCH>